**Section 15- Open Show Rules**

SS Open Rules

* Any steel Small Block engine
* (1) 2bbl carburetor
* 10” MAX width on any tire
* No 3-Link or Late Model type chassis. Must have Stock Front Clip. Clip cars MUST be 2”x3” Steel tubing from 36” behind centerline of front wheels to centerline of rear axle and must go over rear axle.
* No weight rule

Mini Stock Open Rules

* (1) 2bbl carburetor
* 8” MAX width on any tire
* Stock-type suspension
* No weight rule